; This INF file installs the Silicon Image Serial ATA non-Raid driver
; for the SiI 3124 controller on systems using the 64-bit Intel
; Itainium processor.
;
; Copyright (C) 2003 - 2005 by Silicon Image, Inc.
; All rights reserved

[Version]
Signature="$Windows NT$"
Class=SCSIAdapter
ClassGuid={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%SI%
CatalogFile=SI3124.cat
DriverVer=11/29/2005, 1.1.10.0


[SourceDisksNames.ia64]
1="Silicon Image SiI 3124 SATALink Driver Installation Disk",Si3124.inf,\ia64,

[SourceDisksFiles.ia64]
SI3124.sys	= 1
SilSupp.cpl	= 1
SiWinAcc.sys	= 1


[DestinationDirs]
DefaultDestDir	= 12
DllFiles		= 11


[DriverFiles]
SI3124.sys,,,0x20
SiWinAcc.sys,,,0x20

[DllFiles]
SilSupp.cpl,,,0x20


[Manufacturer]
%SI%=SI_HDC,NTia64

[SI_HDC.NTia64]
%PCI\VEN_1095&DEV_3124.DeviceDesc%=SI_3124_XP, PCI\VEN_1095&DEV_3124&SUBSYS_31241095

[ControlFlags]
ExcludeFromSelect.ntx86=*



;; Driver install sections
;;
[SI_3124_XP.NTia64]
Copyfiles=DriverFiles, DllFiles

[SI_3124_XP.NTia64.Services]
AddService=SI3124,0x00000002,SI_3124_Service_Install, Miniport_EventLog_Inst
AddService=SiFilter,0,FilterService_Install

[SI_3124_XP.NTia64.CoInstallers]
Copyfiles=DllFiles
AddReg = SI_3124_CoInstall_AddReg


[SI_3124_CoInstall_AddReg]
HKR,,CoInstallers32,0x00010000,"SilSupp.cpl, CoInstHandler"


[SI_3124_Service_Install]
DisplayName=%SI3124.SvcDesc%
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\SI3124.sys
LoadOrderGroup=Scsi miniport
AddReg=PnPSupport_AddReg
AddReg=PortConfigure_AddReg
AddReg=ProblemDeviceList_AddReg
AddReg=SupportedSubSystemIds_AddReg


[FilterService_Install]
DisplayName=SATALink driver accelerator
ServiceType=1
StartType=0
ErrorControl=0
ServiceBinary=%12%\SiWinAcc.sys
LoadOrderGroup=Filter


; Mark device as supporting Plug & Play on the PCI(5) bus.
[PnPSupport_AddReg]
HKR,Parameters\PnPInterface,5,0x00010001,1


[PortConfigure_AddReg]
HKR,Parameters\Device,NumberOfRequests,0x00010001, 124
HKR,Parameters\Device,MaximumSGList,0x00010001, 33


; List of devices with known configuration issues.
[ProblemDeviceList_AddReg]
HKR,ProblemDevices
HKR,ProblemDevices, %ProblemDev1Name%, 0, %ProblemDev1Value%
HKR,ProblemDevices, %ProblemDev2Name%, 0, %ProblemDev2Value%
HKR,ProblemDevices, %ProblemDev3Name%, 0, %ProblemDev3Value%
HKR,ProblemDevices, %ProblemDev4Name%, 0, %ProblemDev4Value%
HKR,ProblemDevices, %ProblemDev5Name%, 0, %ProblemDev5Value%


; List of controller subsystem IDs to be supported by the SI3124.sys driver.
[SupportedSubSystemIds_AddReg]
HKR,SupportedSubsystemIDs,%PCI\VEN_1095&DEV_3124.DeviceDesc%,0x00010001, 0x31241095


;*************************************************************
;The NT EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,0x00010001,7


[Strings]
SI="Silicon Image"

PCI\VEN_1095&DEV_3124.DeviceDesc="Silicon Image SiI 3124 SATALink Controller"
SI3124.SvcDesc="SiI-3124 SATALink Controller"


ProblemDev1Name="Maxtor 4D060H3                          DAK05GK0"
ProblemDev1Value="MaxMode = UDMA-5"

ProblemDev2Name="HDS724040KLSA80                         KFAOA32A"
ProblemDev2Value="DisableAtaQueueing"

ProblemDev3Name="HDS722525VLSA80                         V36OA6MA"
ProblemDev3Value="DisableAtaQueueing"

ProblemDev4Name="HDS722516VLSA80                         V34OA6MA"
ProblemDev4Value="DisableAtaQueueing"

ProblemDev5Name="Maxtor 7B250S0                          BANC1B70"
ProblemDev5Value="DisableSataQueueing"

